#
CLIMATE CONTROL UNIT CONSTRUCTION [MANUAL AIR CONDITIONER]

id0740001009a2
• A wire-type climate control unit is used with the manual air conditioner.
• The airflow mode selector dial, temperature control dial, fan switch have been enlarged to improve ease of operation.
• The A/C, REC/FRESH and rear defroster switches equipped in the current climate control unit have been relocated to the center panel.

.

1 | Climate control unit
2 | Airflow mode selector dial
3 | Fan switch
4 | Temperature control dial

• A defroster switch into the climate control unit detects when the airflow mode selector dial is turned to DEFROSTER position. When the defroster switch turned on, the center panel starts defroster control. (See Defroster Control.)

.

1 | Climate control unit
2 | Airflow mode selector dial
3 | Defroster switch