#
NO.25 ENGINE STALLS WHEN DRIVING AT SLOW SPEED OR STOPPING [JA5AX-EL]

id050305803000

25 | Engine stalls when driving at slow speeds or stopping
DESCRIPTION | • Engine stalls when brake pedal depressed while driving at low speed or stopping.
POSSIBLE CAUSE | • Malfunction is on engine control side (e.g. Fuel injection control, electronic throttle control system) Note • Before following troubleshooting steps, make sure that Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Go to symptom troubleshooting No.10 "Low idle/stalls during deceleration". (See NO.10 LOW IDLE/STALLS DURING DECELERATION [L8, LF, L3].) • Is engine control system okay? | Yes | Go to symptom troubleshooting No.24 "Engine stalls when shifted to D range, or in R position".
No | Repair or replace any defective parts according to inspection results.
2 | • Verify test results. - If okay, return to diagnostic index to service any additional symptoms. - If malfunction remains, inspect related Service Informations and perform repair or diagnosis. • If vehicle repaired, troubleshooting completed. • If vehicle not repaired or additional diagnostic information not available, replace TCM.