CYLINDER BLOCK DISASSEMBLY (I)

id011000500600

1. Disassemble in the order indicated in the table.

beltze00000009

1 | Oil pan (See Oil Pan Disassembly Note.)
2 | Oil filter cover
3 | Oil filter
4 | Oil cooler
5 | Gasket
6 | Oil filter adapter
7 | Knock sensor
8 | Crankcase ventilation cover
9 | Thermostat
10 | Water pump
11 | Oil strainer
12 | Oil pump
13 | Flywheel (MTX), Drive plate (ATX) (See Flywheel (MTX), Drive Plate (ATX) Disassembly Note.)
14 | Rear oil seal

Oil Pan Disassembly Note

1. Remove the oil pan using a oil pan seal cutter.

e6u110zeb022

Flywheel (MTX), Drive Plate (ATX) Disassembly Note

1. Use the SST to lock the crankshaft against rotation.

beltze00000010